{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":30,"n_cols":7,"rows_kept":30,"cut":false,"hidden":false,"merged":[[1,1,1,6],[0,1,0,6]]}
[]
["1.输入产品类型","2.输入载荷说明（黄色）3.输入每个载荷说明的压力（绿色）"]
["TFC测试","41Bar","59Bar","79Bar","100Bar","121Bar","141Bar"]
["输入压力:",41,59,79,100,121,141]
[]
["222分体外机","夹持1～3台","夹持4～6台","夹持7～12台","夹持12～16台","夹持17～20台"]
["输入压力:",72,89,100,112,124]
[]
["333空调柜机立式","夹持2台","夹持4台","夹持6台","夹持8台","夹持10台","夹持12台"]
["输入压力:",62,76,89,103,117,128]
[]
["444分体柜机内机","夹持1～3台","夹持4～6台","夹持7～12台","夹持12～16台"]
["输入压力:",180,15,90,119]
[]
["555分体柜机外机","夹持1～3台","夹持4～6台","夹持7～12台","夹持12～16台","夹持17～20台"]
["输入压力:",72,89,100,112,124]
[]
["666一体空调柜机","夹持2台","夹持4台","夹持6台","夹持8台","夹持10台","夹持12台"]
["输入压力:",62,76,90,103,117,128]
[]
["777除湿机","夹持1～3台","夹持4～6台","夹持7～12台","夹持12～16台"]
["输入压力:",180,15,90,119]
[]
["888电冰箱","夹持1～3台","夹持4～6台","夹持7～12台","夹持12～16台","夹持17～20台"]
["输入压力:",72,89,100,112,124]
[]
[]
["输入压力:"]
[]
[null,"备注：输入的压力值范围：34～159"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":15,"n_cols":4,"rows_kept":15,"cut":false,"hidden":true,"merged":[]}
["Active-Lang","cn","en","版本说明："]
["TFC ™ - 夹紧力控制","TFC ™ - 夹紧力控制","TFC ™ - Touch Force Control","R1：增加中英文切换按钮"]
["保存数据文件","保存数据文件","Save Data File"]
["1.输入产品类型","1.输入产品类型","1. Enter Product Types"]
["输入压力:","输入压力:","Enter Pressure:"]
["2.输入载荷说明（黄色）","2.输入载荷说明（黄色）","2. Enter Load Description (Yellow)  "]
["3.输入每个载荷说明的压力（绿色）","3.输入每个载荷说明的压力（绿色）","3. Enter Pressure for Each Load (Green)"]
["清空数据","清空数据","Clear Data"]
["您要删除最后几行数据？请输入要删除的行数！ \n \n清空所有数据，请输入9","您要删除最后几行数据？请输入要删除的行数！ \n \n清空所有数据，请输入9","How many rows do you want to delete from last row?\nEnter the quantity of rows you will delete.\n\nDelete all,please enter 9."]
["备注：输入的压力值范围：34～159","备注：输入的压力值范围：34～159","Note: Entering Pressure Range: 34～159"]
[]
["TFC™ - 夹紧力控制为Cascade Corporation 2014版权所有\n\n此工具仅授权用于编程Cascade TFC™夹紧力控制系统。\n\n单击“是”即表示您已阅读并同意这些条款。","TFC™ - 夹紧力控制为Cascade Corporation 2014版权所有\n\n此工具仅授权用于编程Cascade TFC™夹紧力控制系统。\n\n单击“是”即表示您已阅读并同意这些条款。","TFC™ - TOUCH FORCE CONTROL Copyright 2014 By Cascade Corporation\n\nThis tool is licensed solely for programming the Cascade TFC™ TOUCH FORCE CONTROL System.\n\nBy clicking \"Yes\", you agree that you've read and accept these terms."]
["您已拒绝这些条款，此工具将被关闭！","您已拒绝这些条款，此工具将被关闭！","Because you have refused the Terms & Conditions, \nyou will be exited from this tool."]
["3字符文件标识符","3字符文件标识符","3 Character File Identifier"]
["为您的TFC LoadData配置文件输入一个3字符标识符。\n如果您在该进程中运行保存，您将发现系统已为您预先填入该标识符。","为您的TFC LoadData配置文件输入一个3字符标识符。\n如果您在该进程中运行保存，您将发现系统已为您预先填入该标识符。","Enter a 3 character identifier for your TFC LoadData config file. \nIf you run saved during this session, you will find the identifier pre-populated for you."]